**Appendix 7**

**Alignment of X-ray field to light field – Record sheet**

**Year:**

**X-ray equipment ID:**

**Note: The X-ray field to light field must be within ±2% of the SID**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Date:** |  |  |  |  | |
| **Distance between X-ray field and light field (mm). Include the percentage difference to the SID used (positive percentage = extension beyond the light field)** | | | | | |
| **Anode Edge** |  |  |  | |  |
| **Cathode Edge** |  |  |  | |  |
| **Top Edge** |  |  |  | |  |
| **Bottom Edge** |  |  |  | |  |
| **Pass (√) Fail (x)** |  |  |  | |  |
| **Comments:** |  |  |  | |  |